

**VEHICLE DRAIN AND DISCONNECT GUARANTEE**

**NON-HAZARDOUS SHIPMENT**

**MAKE:**   **MODEL:**  **VIN NUMBER:**

**BOOKING NUMBER:**

**CONTAINER NUMBER:**

**SHIPMENT TO:**

THIS IS TO CERTIFY THAT THE VEHICLE(S) PACKED IN THIS CONTAINER HAVE BEEN:  
  
1 COMPLETELY DRAINED OF FUEL AND RUN UNTIL STALLED.   
VEHICLES POWERED BY A FUEL WITH A FLASHPOINT ABOVE THAN 38°C (100.4°F) LIKE DIESEL FUEL MAY CONTAIN UP TO 450l OF FUEL.

2 BATTERIES MUST BE PROTECTED AGAINST SHORT CIRCUITS AND  
 PROPERLY SECURED TO PREVENT MOVEMENT IN ANY DIRECTION.

3 THE VEHICLE(S) ARE PROPERLY BLOCKED AND BRACED TO PREVENT   
 MOVEMENT IN ALL DIRECTIONS WITHIN THE CONTAINER.

4 THE VEHICLE(S) HAVE BEEN INSPECTED FOR SIGNS OF LEAKAGE FROM BATTERIES, FUEL SYSTEM, FUEL CELLS, COMPRESSED GAS CYLINDERS, OR ACCUMULATORS OR ANY OTHER VEHICLE PART.

5 NO DANGEROUS GOODS/HAZARDOUS MATERIALS WHICH ARE NOT PART OF THE VEHICLE ARE IN THE VEHICLE.

I CERTIFY THE ALL OF THE ABOVE HAVE BEEN PROPERLY PREFORMED.

**SIGNATURE:**

**ADDRESS:**

ADDITIONAL NOTES:

THIS VEHICLE(S) ARE ONLY CONSIDERED NON-RESTRICTED (NON-HAZARDOUS) PER 49 CFR 173.220, 176.905 and IMDG Code Special Provision 961 IF **ALL** PROVISIONS ARE MET.

FOR VESSEL SHIPMENTS ONLY.

SSI 3/2016